=== Manual and data ===

ModPack T174-2B Version9 (LS15) of *ieg53i*

Sorry for the English translation, I hope you can read it and understand to some extent...

The time has come, the Version9 is now finished and LS15 fit.
Now there's a load indicator in conjunction with the two grippers
indicative of the weight.
Front window opens and the view through the windows has been improved.
All three engine doors open.
Motor shafts were animated and rotate the engine speed dependent.
The supports are now not only movable extensions, but now also have the function
for support.
The device support automatically adjusts to the both arm movements and is always perpendicular.
Except in transport mode!
It was fitted with a windshield wiper, which automatically wipes the rain.
Furthermore, a transport function was blocked.
This Funktiuon should only in connection with one of the two grippers in the open condition
and the wood grips are used in the closed state.
It serves the following purpose, the excavator to drive in this position for a longer distance,
or to go on a low loader and transported with this.
Transport function for rack and hooks suitable!
Complete steering linkage was fully animated, also the driver.
All displays in the cockpit were fully animated and show the current state of.
Handbrake and manualIgnition installed.
All pedals and levers move to the respective functions.
Speed gearbox with four forward and reverse gear installed.
Clutch pedal disengages the clutch when shifting gears.
Mirror active in the Camera mode cockpit / cabin.
Camera installed on the boom.
Thus, three camera views with key C are selectable through.
================================================== ========

!!! The downloaded zip file not unpack !!!

!!! Copy the mod folder and do not rename !!!

In the mod folder must be:

T174_2B_V9_LS15

================================================== ==================
Giants editor 6.0.0 and LS15 Patch 1 or later is required!
================================================== ==================


multiplayer supported / MP-capable
Grippers are AlternativeTipping fit (within the meaning of placeable clusters)
Modpack is not MR-compatible
-------------------

Technical data:

Mobile Crane Progress T 174-2B
2 VD 14.5 / 12-1 SRL 25kW / 34PS
VEB Weimarwerk (DDR)
Produced from 1965 to 1972 as T174 / T174-1 8914 pieces built.
From 1972 to 1974 built as T174-2 ab1974 T174-2A From 1988 T174-2B 18924 pieces.
Revision of the lower trolley and cultivation of a hydraulic support
whereby the carrying capacity was increased to 2,5to.
It was also an air-pressure-assisted brake, trailer hitch and
a load indicator and an air suspension seat installed.
Previous model loader Weimar T172 with Cable
Successor progress T185
----------------------------------

T174-2 in yellow, blue and green
Purchase price € 12,900 Maintenance / day 40, - €

shovel claw
Purchase price 900, - € Maintenance / day 19, - €

fork claw
Purchase price 900, - € Maintenance / day 19, - €

woodclaw
Purchase price 900, - € Maintenance / day 19, - €

hook
Purchase price 150, - € Maintenance / day 4, - €

balegrab
Purchase price 1200 - € Maintenance / day 23, - €

frame
Purchase price 700, - € Maintenance / day 16, - €
---------------------------------------

data:

excavator
Fuel capacity 500 liters

shovelGripper
Capacity in 1800
Multi Fruit
charge of
wheat barley rape maize potato sugarbeet grass_windrow dryGrass_windrow
wheat_windrow barley_windrow forage silage chaff manure woodchips

grabGripper
Capacity in 1800
charge of
manure silage grass_windrow dryGrass_windrow wheat_windrow barley_windrow

woodGripper
load of logs

hook
= Consumption of all devices with the attacherJoint joint type "trailer"
e.g. Tow bars, chains, cables ** also ** Trailer

baleGrab
Attacks round and square bales of all kinds
What was once captured not fall out!
*** For front loader used conditionally ***

frame
Ball-nose pliers and FL-On Devices
(Forks blades grab pallet forks)
Rotatable device support
----------------------

control:

                             keyboard                  mouse
Support                      leftCtrl + v / b          left + right y-axis
Devices Turner on the boom   leftShift + v / b         left + right xAxis
Turn excavator               k / m                     left xAxis
Main arm                     n / j                     left y-axis
Boom                         leftShift + n / y         right y-axis
Gripper open / close         leftShift + k / m         right xAxis
Turn recording *frame*       leftCtrl + k / m          center xAxis
Recording on / off *frame*   leftCtrl + n / y          center yAxis
Pliers open / close          leftShift + k / m         right xAxis
Work light front boom        F-F    or   NumPad6
Work light rear              F-F-F  or   NumPad5
Lighting                     F
Rotating Light / Rul         Pos1
Left turn signal             NumPad 1
Right turn signal            NumPad 3
Warning lights               NumPad 2
horn                         0
Driver's door open / close   spacebar, then the respective marker selection is displayed * * follow it.
Motordoor1 open / close      spacebar, then the respective marker selection is displayed * * follow it.
Motordoor2 open / close      spacebar, then the respective marker selection is displayed * * follow it.
Motordoor3 open / close      spacebar, then the respective marker selection is displayed * * follow it.
Front window open / close    spacebar, then the respective marker selection is displayed * * follow it.
                             Re-press the spacebar disables the markings.
Transport mode               X   Device selection before on excavator and only in conjunction with one of the gripper
Wipers on / off              automatically when it rains
Motor shafts                 automatically controlled by engine speed
-------------------------------------------------- -----------

Engine start button with NupadEnter or W

Take the excavator is only possible if, following the "boarding" / vehicle choice
the engine to "full tour" is running. Approximately 10 sec

Loess before driving handbrake.

With extended support not drive!

During storage and subsequent re-start a savegame
remains the transport function, if it was triggered off condition.

Coupling of the individual devices:

Use the rotary part which the boom is above the desired device
move and, if necessary, turn the rotator with keyboard or mouse
until the Hitchsymbol appears.
When coupling at the gun where appropriate, the turners
press the frame.
It is important to ensure that the particular device that moves or off
should also be coupled in scheme (key G) is selected.
----------------------

Mod has been tested on the Bjorn Holm-standard cards and different computers.

Mod is log error-free and does not cause "missingl10n" warnings.

-------------------------------------------

Credids:

Excavators = new construction and re-writing the scripts and xml
           and conversion to LS15 * * ieg53i

Shuttle = new construction and xml * * ieg53i

Woodclaw = new construction / reconstruction of OrginalLS15 * * ieg53i

Hook = new construction and xml * * ieg53i

Frame = new construction and xml * * ieg53i

Pliers and xml = new ieg53i * *

Engine sound courtesy of * * Falcrum
Modulation and partially re-recording of .wav files * * ieg53i

Scripts zylinderV2 courtesy of * model * eicher

Gears teamwork ieg53i and Bavarian michel
--------------------

Note:

Modifications and reinstatement is strictly prohibited!
Please ask for authorization via PM!
Parts that are included in this mod, not from === === ieg53i
sodern were created by the modders are listed in Credids
modified and only ieg53i.
I ask specifically for your attention!

All the modders listed in Credids and unintentionally unnamed
is herewith my thanks for the permits.
I would also like bassaddict at * * thank sincerely
without his help and advice Währe this mod probably not have arisen.

And now wishes good gaming with this mod

=== === ieg53i

PS .: Who finds spelling errors, they may keep!

Errors and misstatements reserved!

Another one for the complainers and alls:
Who does it better, which should send yourself a mod and then on his own mistakes
complain about. Perhaps such a one is then dahiner how much time it takes to complete any
write a mod and how much error there can undermine a.
Who does not like this mod, either not download or delete the mod folder.
Relevant information or corrections are welcome any.
Stupit questions or comments ore less.