Hi All

Model: Knagsted
Textures: Knagsted
Script: Knagsted
Ingame testing: Knagsted


Thankyou for downloading my 2009 GIANTS MODCONTEST entry: The John Deere 1890 airseeder and John Deere 1910 aircart for LS 2009. 
This is a aircart and seeder that supports the following graintypes: wheat barley oat soybean pea rice rape mohn and fertilizer

NOTE: The 1890 airseeder must be attached behind the John deere 1910 Aircart to work correctly.




SUPPORTED SEED TYPES:
wheat barley oat soybean pea rice rape mohn and fertilizer




Installation:
Place the JDAirseeder.zip, JDAirseederLowPoly.zip and JDAircart.zip file in the "C:\Documents and Settings\[user]\Documents\My Games\FarmingSimulator2011\mods" folder
NOTE: The JDAirseederLowPoly.zip seeder is i slightly less heavy version of the seeder in regards to graphics. 
Buy this in game if you have trouble running the more detailed JDAirseeder.zip.





FEATURES and USERGUIDE:
This section explains you how to use the airseeder and aircart. Please take your time to read it carefully, 
so you will fully understand how to operate the model and use it properly.

-FOLD AND UNFOLD SEEDER
Fold and unfold the seederbar by pressing [Y] and [U]. Please note that the seeders must be raised [N] before you can fold.
You cannot lower the seeders unless the seederbar is fully unfolded.

-NO TILL
When YOU CONTROL the tractor where the seeder and aircart is attached to, the seeder will function as a "No Till/Direct drill". 
This means that no plowing/harrowing is needed before you can seed. Hence, you can seed directly into the stubble with the 1890 seeder.
This saves you a lot of time, fuel and money.
Lower and raise the seederbar uning [N]

-AIRFLOW
Airseeders work via airflow. The seed and fertilizer is distributed to the seeder units via this airflow, 
so in order to be able to sow, you need to turn on the airflow fan by pressing [b].

-MANUAL FILL
In order to sow a field, the aircart must be loaded with seed. To do this use the swingable auger:
1: Press [K] to swing auger to the prefered fill position (Fill rear, Fill front, Empty front, Empty rear and transport).
   If the HUD is activated [0], it will tell you the current and next position of the grain auger.
2: Open the tank lids [o]
3: (FILLING) The load position of the auger must be close to a trailer holding one of the supported seed types. 
   For guidance icon, activate the HUD[0]. When the auger filling station is in a proper position for loading, the icon will show.
   If you cant get the icon to show, try to drive a bit around to reposition the aircart in relation to the trailer holding the seed.
   The filling station of the auger should be positioned underneath the sides of the trailer for it to start loading.
4: Turned on the auger[J]. If the filling station of the auger is close enough to the trailer, 
   and the aircart tank to fill (front or rear) is empty or holds the same seed type as the trailer the tank will start filling.
   NOTE: If turned on, the grainauger will automatically turn off when swinging it to the next position [G].
5: Only one seed type is supported at a time in total. E.g front tank can not hold peas while rear tank holds wheat.
6: Fertilizer and seed is supported at the same time. E.g. front tank can hold fertilizer while rear tank holds wheat.

-MANUAL EMPTY
You are done sowing your field, but the aircart still isn't empty. What do you do? -You empty the cart into a trailer:
1: Press [K] to swing auger to the prefered unload position (Fill rear, Fill front, Empty front, Empty rear and transport)
   If the HUD is activated [0], it will tell you the current and next position of the grain auger.
2: (EMPTYING) The unload position of the auger must be close to a trailer that is empty or holds the same seed type as the tank you want to empty. 
   For guidance icon, activate the HUD[0]. When the auger unload position is positioned properly over the trailer, the icon will show.
   If you cant get the icon to show, try to drive a bit around to reposition the aircart in relation to the trailer you want to unload into.
   The unload position of the auger must be positioned within the four sides of the trailers holding area for it to start unloading.
3: Turned on the auger[J]. If the unload position of the auger is close enough to the trailer, 
   and the trailer to unload into is empty or holds the same seed type as the tank you want to unload, the tank will start to empty.
   NOTE: If turned on, the grainauger will automatically turn off when swinging it to the next position [K].
4: The trailer you want to unload into must support the graintype you are unloading. 

-FERTILIZER AND SEED
The aircart has two tanks that fill individually with any of the graintypes listed above. Please note that the cart can only hold 
one type of seed in both tanks or it can hold one type of seed in one tank and fertilizer in another tank.
I recommend you use the front tank for fertilizer and the rear tank for seed if you choose to run a Fertilizer/Seed configuration.
If one tank holds fertilizer and the other holds seed, the airseeder will seed and fertilize the ground in the same go.

-MARKERS
By default, the markers of the seeder shift sides automatically every time you lower the seeder. You can at any time override this shift using
the marker position keys: [KP1] left marker, [KP2] both markers retracted and [KP3] right marker. This way your markers will 
be extended to the side you want them to be and will hereafter shift in accordance to the that side. 
The automatic marker shift can be deactived/activated using key [KP0].
When the airseeder and cart is hired, the markers will not extend automatically.

-HIRABLE
When attached to the John Deere 1910 aircart, the 1890 is hirable if the tractor pulling the implements is hirable.
Please note that if you want to use the seeder as a hired tool, the field you want to sow must be plowed or cultivated in advance.
(I know this goes against what I wrote in the NO TILL section above, but its nessesary as the LS2009 Artificial Inteligence (Helper function) 
otherwise won't know where to steer).
When the aircart no longer holds any seed the helper will automatically stop working.




FUNCTION KEYS:
Attach seeder/aircart:				q
Lower/lift seeders:				n
Unfold to workposition:				u
Fold to transport:				y
Cycle HUD:					0 (number)
Swing grain auger to next predefined position:	k
Turn on grain auger:				j
Open tank lids:					o (letter)			
Turn airflow on/off:				b
Auto markers disable/enable:			0 (Keypad)
Left marker:					1 (keypad)
Markers unfolded/transport:			2 (keypad)
Right marker:					3 (keypad)
Helper on/off(AI):				h



I hope you will enjou the Model as much as I've enjoyed creating it :-)

Best Regards
Knagsted
